##### New_DOE_Logo_Color_042808CCSI_color_CS3_TM_300dpi.png



**Intellectual Property Management Plan**

**February 28, 2011**

MFIX SIMULATIONS FOR

1 Mega Watt Pilot Device

Installation Guide and User Manual

Version 2.0.0

March, 2018

Copyright (c) 2012 - 2018

**Copyright Notice**

1MW CFD was produced under the DOE Carbon Capture Simulation Initiative (CCSI), and is copyright (c) 2012 - 2018 by the software owners: Oak Ridge Institute for Science and Education (ORISE), Los Alamos National Security, LLC., Lawrence Livermore National Security, LLC., The Regents of the University of California, through Lawrence Berkeley National Laboratory, Battelle Memorial Institute, Pacific Northwest Division through Pacific Northwest National Laboratory, Carnegie Mellon University, West Virginia University, Boston University, the Trustees of Princeton University, The University of Texas at Austin, URS Energy & Construction, Inc., et al.. All rights reserved.

NOTICE. This Software was developed under funding from the U.S. Department of Energy and the U.S. Government consequently retains certain rights. As such, the U.S. Government has been granted for itself and others acting on its behalf a paid-up, nonexclusive, irrevocable, worldwide license in the Software to reproduce, distribute copies to the public, prepare derivative works, and perform publicly and display publicly, and to permit other to do so.

**License Agreement**

1MW CFD Copyright (c) 2012 - 2018, by the software owners: Oak Ridge Institute for Science and Education (ORISE), Los Alamos National Security, LLC., Lawrence Livermore National Security, LLC., The Regents of the University of California, through Lawrence Berkeley National Laboratory, Battelle Memorial Institute, Pacific Northwest Division through Pacific Northwest National Laboratory, Carnegie Mellon University, West Virginia University, Boston University, the Trustees of Princeton University, The University of Texas at Austin, URS Energy & Construction, Inc., et al. All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

1. Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
2. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.
3. Neither the name of the Carbon Capture Simulation Initiative, U.S. Dept. of Energy, the National Energy Technology Laboratory, Oak Ridge Institute for Science and Education (ORISE), Los Alamos National Security, LLC., Lawrence Livermore National Security, LLC., the University of California, Lawrence Berkeley National Laboratory, Battelle Memorial Institute, Pacific Northwest National Laboratory, Carnegie Mellon University, West Virginia University, Boston University, the Trustees of Princeton University, the University of Texas at Austin, URS Energy & Construction, Inc., nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

You are under no obligation whatsoever to provide any bug fixes, patches, or upgrades to the features, functionality or performance of the source code ("Enhancements") to anyone; however, if you choose to make your Enhancements available either publicly, or directly to Lawrence Berkeley National Laboratory, without imposing a separate written license agreement for such Enhancements, then you hereby grant the following license: a non-exclusive, royalty-free perpetual license to install, use, modify, prepare derivative works, incorporate into other computer software, distribute, and sublicense such enhancements or derivative works thereof, in binary and source code form. This material was produced under the DOE Carbon Capture Simulation

**Revision Log**

|  |  |  |
| --- | --- | --- |
| Version Number | Release Date | Description |
| Version 2015.01.0 | 01/15/2015 | Initial Release |
| Version 2015.01.1 | 03/02/2015 | ONEMWCFD-6 |
| Version 2015.01.2 | 06/19/2015 | ONEMWCFD-7 |
| Version 2015.01.3 | 07/07/2015 | ONEMWCFD-7 |
| Version 2015.01.4 | 11/06/2015 | ONEMWCFD-8 |
| Version 2.0.0 | 03/31/2018 | Initial Open Source release |

Table of Contents

[1. Installation 1-1](#_Toc506304351)

[1.1. Prerequisites 1-1](#_Toc506304352)

[1.2. Third Party Software 1-1](#_Toc506304353)

[1.3. Product Installation 1-1](#_Toc506304354)

[Build custom code for 1MW system simulations 1-2](#_Toc506304355)

[2. simulations 2-2](#_Toc506304356)

[2.1. pre-processing 2.1-3](#_Toc506304357)

[2.2. Post-processing 2.2-4](#_Toc506304358)

[3. references 3-4](#_Toc506304359)

# Installation

CCSI 1MW simulations are custom MFIX simulations. For that reason, the general installation procedure in this user manual follows that of MFIX [1]. In this session, only the 1MW specific installation procedure will be covered in details, leaving the general MFIX steps referring to the MFIX manual.

## Prerequisites

The hardware and software prerequisites follow exactly that of MFIX [1].

## Third Party Software

Open-source, multi-platform data analysis and visualization application ParaView is recommended for the MFIX simulation post-processing purpose. Users can download ParaView software online from <http://www.paraview.org/>.

Users can choose other similar visualization tools (for example, *Visit*) for the post-processing need.

## Product Installation

This session will only describe the steps to build CFD models for 1MW CFD simulations. It is assumed that users have downloaded MFIX source files of version 2014-1, set environment variables and alias, and built mfix.exe on their chosen platform under $InstallDir/mfix/model. Users can build either a serial version or a parallel version of mfix.exe following instructions in [1].

Download release archive from GitHub from the following URL: <https://github.com/CCSI-Toolset/1mw_cfd/releases>

Unzip the file, you will get three directories: src, docs, and scripts

The following files are under src directory:

calc\_mu\_s.f

allocate\_arrays.f

check\_data

check\_data\_30.f

drag\_gs.f

drag\_ss.f

ic\_mod.f

init\_namelist.f

namelist.inc

rrates0.f

set\_ic.f

solve\_energy\_eq.f

source\_u\_s.f

source\_v\_s.f

species.inc

usr0.f

usr\_init\_namelist.f

usr\_mod.f

usrnlst.inc

usr\_rates.f

Note that check\_data is a subdirectory containing two files:

check\_bc\_inflow.f

check\_initial\_conditions.f

This Installation Guide/User Manual file CCSI\_Software\_Install\_1MW.docx is available under

docs directory.

The script files, which are useful for pre- and post-processing of the 1MW CFD simulations, are under scripts directory:

PP1MW.pl

PostMfix.pm

MyMath.pm

Util.pm

mfix.dat

mfix.mod

Modify1MW2.pl

RunCase

RunAll.pl

ProcessAll.pl

## Build custom code for 1MW system simulations

The 1MW system custom code should be built on top of MFIX official release of September 2014 (Version 2014-1). This release can be downloaded from MFIX web site:

[https://mfix.netl.doe.gov/mfix/download-mfix](https://mfix.netl.doe.gov/mfix/download-mfix/)

The installation from the official release should create and populate content under $InstallDir, i.e., $HOME/mfix.

Create a directory for 1MW, e.g., $HOME/CCSI/1MW, and copy all the custom source code files to the directory. In the 1MW directory type “sh $InstallDir/model/make\_mfix” and follow instructions on [1] to build the model. The build process will compile object files and generate a custom mfix.exe in directory $InstallDir/mfix/model. Upon successful compilation, mfix.exe is also copied to $HOME/CCSI/1MW.

# simulations

A sample model input file mfix.dat for the 1MW simulation is included in the scripts directory. Users can choose to run serial or parallel version of the CFD simulation. For more details, please refer to [1] for general MFIX simulations.

The 1MW simulations consist of large number of simulations with 14 varying parameters with values designed by the uncertainty quantification (UQ) analysis. In the following, a brief instruction is provided to summarize the automation procedure that facilitates the simulations and post-processing needs.

# pre-processing

For both pre-processing and post-processing, the user should copy the Perl script files to $HOME/*bin* directory that is included in PATH variable:

PP1MW.pl

PostMfix.pm

MyMath.pm

Util.pm

Modify1MW2.pl

RunAll.pl

ProcessAll.pl

The user should create a run directory (i.e., *$RunDir=$HOME/1MWRuns*) and copy the following files to the run directory:

mfix.dat

mfix.mod

RunCase

UQ\_351\_design\_32D\_1MW.txt

For all Perl script files, the user must check and change the first line to the local Perl setting unless the file starts with

#!/usr/bin/env perl

Change this line accordingly to the user’s Perl script bin directory

use lib "/pic/people/kevinlai/bin";

For the run script *RunCase*, the user must check and modify the following to conform to the local setting:

1. Linux/Unix bash setting
2. Module loading: make it consistent with the compiler choice
3. email address
4. location of mfix.exe
5. limit on the total run time of the job allocation
6. Command for a parallel run: currently it is “mpirun –np” but the user must check with his/her own Linux system setting.
7. If the number of processors is changed in the model file mfix.dat (i.e., NODESI \* NODESJ \* NODESK), make sure that the run script is modified to match the new value.
8. If mfix.exe is built serial, make sure NODESI= NODESJ=NODESK=1 in mfix.dat

After the modifications, run the script in *$RunDir:*

*./Modify1MW2.pl*

This script does the following:

1. Create 351 sub-directories, Case001 to Case351
2. Copy mfix.mod to mfix.dat at each case sub-directory
3. Modify mfix.dat according to the parameter settings defined in *UQ\_351\_design\_32D\_1MW.txt*
4. Copy file *RunCase* to *RCasexxx* sub-directory (i.e., *RCase012*)

The user can go to each case sub-directory and run the batch script *RCasexxx*. Alternatively, the user can run all simulations by

*./RunAll.pl*

# Post-processing

The user can choose any post-processing tool to analyze the simulation result, e.g., the official MFIX post-mfix script or the open-source ParaView software.

Alternatively, a Perl script PP1MW.pl provided in this product can be used to automated the post-processing. Go to the simulation directory, e.g., *Case012* and run

*PP1MW.pl –o result\_file*

The data in the result file should be self-explanatory. It prints all the QOIs (quantity of interest) for the 1MW system simulations.

# references

[1] MFIX – Multiphase Flow with Interphase eXchanges, Version MFIX-2014-1. Download available for members: <https://mfix.netl.doe.gov/mfix/download-mfix>